ROOF HOOK REMOVAL/INSTALLATION

id091600810500

1. Fully close the power retractable hardtop.

2. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

3. Open the cable case cover and disconnect the cable while pressing the cable in the direction of the arrow. (See Roof Hook Install Note)

amxzzw00002093

4. Remove the bolts.

amxzzw00002094

5. Remove the screw.

6. Remove the roof hook.

7. Remove the screws.

amxzzw00002095

8. Pull up the cover and remove the hook.

9. Remove the cover.

10. Install in the reverse order of removal.

Roof Hook Install Note

1. Securely fix the 3 cable-side grooves to the cable case.

amxzzw00002096