INSTANT MOBILITY SYSTEM OUTLINE

id021200629600

• An instant mobility system has been provided for the vehicle not equipped with the run-flat tire instead of a temporary spare tire. This system enables temporary repair of a puncture without tire removal.
• The instant mobility system is located in trunk compartment and includes the following:

amxzzn00000256

  ― Repair agent
  ― Repair agent filler hose
  ― Air compressor
  ― Tire valve core
  ― Tire valve core tool
  ― Instruction manual
  ― Speed limit label
  ― Filled tire indication label

• The accessory socket (12 V DC) is used as an input power source for the air compressor and the compressor plug includes a 10 A fuse.

  Note
  • The expiration date of the repair agent is printed on the repair agent bottle. Do not use the repair agent if it has passed the expiration date.
  • Dispose of repair agent according to local waste disposal law.
  • The repair agent consists of the following ingredients:
    ― Deproteinized natural rubber latex
    ― Emulsified adhesive resin
    ― Propylene glycol