CLUTCH PEDAL POSITION (CPP) SWITCH INSPECTION [L8, LF]

id0140i7801600

1. Verify that the CPP switch is installed properly.

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the negative battery cable.

4. Disconnect the CPP switch connector. (See CLUTCH PEDAL REMOVAL/INSTALLATION.)

5. Inspect for continuity between the CPP switch terminals using an ohmmeter.

am3uuw00002798

  • If not as specified, replace the CPP switch.
  (See CLUTCH PEDAL REMOVAL/INSTALLATION.)

Specification

Measured condition | Clutch pedal position | Continuity
--- | --- | ---
Rod pushed | Clutch pedal released | Continuity detected
Except above | Clutch pedal depressed | No continuity