PROPELLER SHAFT REMOVAL/INSTALLATION

id031500800300

1. Remove the member, the exhaust pipe and the main silencer. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

2. Remove in the order indicated in the table.

amxzzw00001310

1 | Bolt, nut
2 | Propeller shaft (See Propeller Shaft Removal Note.) (See Propeller Shaft Installation Note.)

3. Install in the reverse order of removal.

Propeller Shaft Removal Note

  Caution
  • When replacing with a new propeller shaft, mark the companion flange to match the position of the tag on the propeller shaft.

1. Before removing the propeller shaft, make alignment marks on the yoke and differential companion flange.

amxzzw00002388

2. Install the SST to the extension housing.

amxzzw00001311

Propeller Shaft Installation Note

1. Align the marks and install the propeller shaft.

2. When installing a new propeller shaft, align the differential companion flange mark with the tag on the propeller shaft and assemble.

amxzzw00002389