UPPER BLOCK REMOVAL/INSTALLATION

id092100801800

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the main fuse block cover.

4. Remove in the order indicated in the table.

e5u921zw5002

1 | Nut
2 | Connector
3 | Upper block (See Upper Block Removal Note)

5. Install in the reverse order of removal.

Upper Block Removal Note

1. Press and remove the tabs on main fuse block at the positions indicated by the arrows.

e5u921zw5003

2. Raise the upper cylinder block and remove it.