AIR DIST (DISTRIBUTION) UNIT CONSTRUCTION

id071100638500

• Composed of the following parts:

  ― Airflow mode actuator
  ― Airflow mode main link
  ― Airflow mode door

amxzzn00000331

Airflow Mode Door Operation

• The airflow mode doors move to the OPEN-VENT, OPEN-BI-LEVEL, OPEN-HEAT, VENT HEAT, DEF/HEAT or DEFROSTER position, depending on the position of the airflow mode control dial. As a result, the airflow mode changes.

amxzzn00000626

Airflow Distribution

AIRFLOW MODE | AIRFLOW RATE (%)
--- | ---
VENT | WAIST | HEAT | DEFROSTER
DRIVER-SIDE | PASSENGER-SIDE | DRIVER-SIDE | PASSENGER-SIDE | DRIVER-SIDE | PASSENGER-SIDE | DRIVER-SIDE | PASSENGER-SIDE
SIDE | CENTER | CENTER | SIDE | SIDE | CENTER | CENTER | SIDE
OPEN-VENT | 21.25 | 21.25 | 21.25 | 21.25 | 7.5 | 7.5 | – | – | – | – | – | –
OPEN-BI-LEVEL | 12.5 | 12.5 | 12.5 | 12.5 | 7.5 | 7.5 | 17.5 | 17.5 | – | – | – | –
OPEN-HEAT | – | – | – | – | 12.5 | 12.5 | 25 | 25 | 2.5 | 16.25 | 2.5 | 3.75
VENT | 25 | 25 | 25 | 25 | – | – | – | – | – | – | – | –
HEAT | – | – | – | – | – | – | 35 | 35 | 4.5 | 3 | 19.5 | 3
DEF/HEAT | – | – | – | – | – | – | 25 | 25 | 7.5 | 7.5 | 27.5 | 7.5
DEFROSTER | – | – | – | – | – | – | – | – | 15 | 20 | 50 | 15