KNOCK SENSOR (KS) REMOVAL/INSTALLATION [L8, LF]

id0140i7802900

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the dynamic chamber. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)

4. Disconnect the KS connector.

5. Remove the KS installation bolt, then remove the KS.

e5u140zw5k01

6. Install in the reverse order of removal.

  KS tightening torque

  16—24 N·m {1.7—2.4 kgf·m, 12—17 ft·lbf}