TRANSMISSION/TRANSAXLE SPECIFICATIONS

id050000100600

Item | Specification
--- | ---
Transmission type | SJ6A-EL
Gear ratio | 1GR | 3.538
2GR | 2.060
3GR | 1.404
4GR | 1.000
5GR | 0.713
6GR | 0.582
Reverse | 3.168
ATF | Type | JWS3309
Capacity (Approx. quantity) (L {US qt, lmp qt}) | 7.4 {7.8, 6.5}
Torque converter stall torque ratio | 2.00
Hydraulic system (Number of drive/driven plates) | C1 clutch | 4/5
C2 clutch | 5/5
C3 clutch | 4/4
C4 clutch | 4/4
B1 brake | 3/3
B2 brake | 4/3
B3 brake | 3/4
B4 brake | 5/5
Front planetary gear (Number of teeth) | Sun gear | 33
Pinion gear (inner) | 19
Pinion gear (outer) | 18
Ring gear | 75
Middle planetary gear (Number of teeth) | Sun gear | 26
Pinion gear | 20
Ring gear | 66
Rear planetary gear (Number of teeth) | Sun gear | 26
Pinion gear | 20
Ring gear | 66

• Example of automatic transaxle specifications. (MX-5 (NC) specifications)