EGR VALVE INSPECTION [L8, LF]

id0116a3801100

Resistance Inspection

1. Disconnect the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the EGR valve connector. (See EGR VALVE REMOVAL/INSTALLATION [L8, LF].)

4. Measure the resistance between the EGR valve terminals.

amxzzw00000840

EGR valve terminal | Resistance (ohm)
--- | ---
C—E C—A D—B D—F | 12—16

  • If not within the specification, replace the EGR valve. (See EGR VALVE REMOVAL/INSTALLATION [L8, LF].)