AMBIENT TEMPERATURE SENSOR REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER]

id0740a1803200

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the under cover.

4. Remove in the order indicated in the table.

amxzzw00000979

1 | Ambient temperature sensor connector
2 | Ambient temperature sensor

5. Install in the reverse order of removal.