LOWER PANEL REMOVAL/INSTALLATION

id091700453900

L.H.D.

1. Pull the lower panel outward and detach clips A and tab B.

amxzzw00001397

2. Turn the lower panel downward and remove the tabs C.

3. Remove the lower panel.

4. Install in the reverse order of removal.

R.H.D.

1. Pull the lower panel outward and detach clips A.

amxzzw00001398

2. Turn the lower panel downward and remove the tabs B.

3. Remove the lower panel.

4. Install in the reverse order of removal.