BELTLINE MOLDING REMOVAL/INSTALLATION

id091600807300

1. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Front seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (8) Seat belt set plate (See SEAT BELT REMOVAL/INSTALLATION.)

  (9) Seat back crossmember assembly (See SEAT BACK CROSSMEMBER ASSEMBLY REMOVAL/INSTALLATION.)

  (10) Rear side trim (See REAR SIDE TRIM REMOVAL/INSTALLATION.)

  (11) Rear package trim (See REAR PACKAGE TRIM REMOVAL/INSTALLATION.)

  (12) Side shelf (See SIDE SHELF REMOVAL/INSTALLATION.)

  (13) Seat belt upper anchor installation bolt (See SEAT BELT REMOVAL/INSTALLATION.)

  (14) Convertible top (See CONVERTIBLE TOP REMOVAL/INSTALLATION.)

2. Remove the fasteners.

e5u916zw5005

3. Remove the beltline protector.

4. Remove the nut and bolts.

5. Remove the beltline molding.

6. Install in the reverse order of removal.