PID/DATA MONITOR TABLE [ACTIVE BONNET]

id0802f1081000

PID name (definition) | Unit/Operation | Operation Status (Reference) | Terminal
--- | --- | --- | ---
DHS_WL (Active bonnet warning light condition) | Lamp_Off/Lamp_On | • Active bonnet warning light is not illuminated: Lamp_Off • Active bonnet warning light is illuminated: Lamp_On | 2M, 2O
RES_ACTU1 (Active bonnet actuator (RH) resistance) | ohm | Continuous: 1.63―7.60 ohm | 1A, 1C
RES_ACTU2 (Active bonnet actuator (LH) resistance) | ohm | Continuous: 1.63―7.60 ohm | 1G, 1E
RES_PCD_BAR (Partially disconnected detection bar resistance (All connector total)) | ohm | • Connector connected: 100 ohms or less • Connector partially disconnected: 20 kilohms or more | 1a, 1b, 2a, 2b, 3a, 3b
VPWR_IGA (IG1 voltage value) | V | • Ignition is switched ON: B+ • Ignition is switched to LOCK: 1.0 V or less | 3A