TRANSMISSION OIL INSPECTION [M15M-D]

id051110247800

1. Position the vehicle on level ground.

2. Remove the Insulator (except L8). (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].)

3. Remove the check plug A.

amxzzw00000496

4. Verify that the oil is at the brim of the check plug hole as shown.

  • If it is low, add the specified oil from the check plug hole.

  Specified oil grade

  API Service GL-4 or GL-5

  Specified oil viscosity

  All season: SAE 75W-90
  Above 10°C {50°F}: SAE 80W-90

5. Install the new check plug A.

  Tightening torque

  A: 25—39 N·m {2.6—3.9 kgf·m, 19—28 ft·lbf}

6. Install the Insulator (except L8). (See TRANSMISSION REMOVAL/INSTALLATION [M15M-D].)