DLC-2 CONSTRUCTION [DYNAMIC STABILITY CONTROL (DSC)]

id0402b2180800

• A connector (DLC-2) conforming to International Organization for Standardization (ISO) standards has been added.
• Shape and terminal arrangement as stipulated by the ISO 15031-3 (SAE J1962) international standard has been adopted for this connector.The 16-pin connector consists of a CAN_H (HS) terminal, CAN_L (HS) terminal, GND1 terminal, GND2 terminal, and B+ terminal.

amxzzn00000124

Terminal | Function
--- | ---
CAN_L (HS) | Serial communication Lo terminal (HS)
CAN_H (HS) | Serial communication Hi terminal (HS)
GND1 | Body ground terminal
GND2 | Serial communication ground terminal
B+ | Battery power supply terminal