HAZARD WARNING SWITCH REMOVAL/INSTALLATION

id091800470100

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the side wall. (See SIDE WALL REMOVAL/INSTALLATION.)

4. Remove the center panel unit. (See CENTER PANEL UNIT REMOVAL/INSTALLATION.)

5. Remove the globe compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

6. Remove the decoration panel (passenger’s side). (See DECORATION PANEL REMOVAL/INSTALLATION.)

7. Remove in the order indicated in the table.

amxzzw00001096

1 | Screw
2 | Hazard warning switch connector
3 | Hazard warning switch

8. Install in the reverse order of removal.