STARTING PROCEDURE FOR ON-BOARD DIAGNOSTIC TEST MODE [HANDS-FREE TELEPHONE (HF/TEL) SYSTEM]

id0902g0358300

  Note
  • All DTCs displayed in the on-board diagnostic test mode should be entered in the Audio Repair Order Form

1. Turn the ignition switch to the ACC or ON position.

2. Turn the audio unit power to OFF.

3. While pressing the POWER/VOLUME switch, simultaneously press the H/PRESET switch 1 and the PRESET switch 6 for 3 s or more.

amxzzw00002468

  Note
  • If several DTCs are in the memory, they can be displayed using the SEEK/TRACK switch (up or down).

  amxzzw00001109

4. To stop the on-board diagnostic test mode, turn the ignition switch to the LOCK position.