No.3 THE PASSENGER'S SIDE POWER WINDOW IS INOPERATIVE [POWER WINDOW SYSTEM]

id0903a0870100

3 | The passenger’s side power window is inoperative
POSSIBLE CAUSE | • power supply circuit malfunction ― Open or short circuit in wiring harness between power window main switch and passenger’s side power window motor • Power window main switch malfunction • Passenger’s side power window motor malfunction • Passenger’s side power window regulator malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Turn the ignition switch to the ON position. • Operate the driver’s side power window using the power window main switch. • Does the power window operate properly? | Yes | Go to the next step.
No | Go to the symptom No.4 ALL POWER WINDOWS ARE INOPERATIVE [POWER WINDOW SYSTEM] troubleshooting procedure.
2 | • Measure the voltage at the power window main switch. (power window motor output terminal) while operating the passenger’s side power window using the power window main switch. • Is the voltage B+? L.H.D. model (Auto on both driver and passenger side): Open: terminal F/close: terminal D L.H.D. model (Auto on driver side only): Open: terminal D/close: terminal A R.H.D. model: Open: terminal J/close terminal I | Yes | Go to the next step.
No | Replace the power window main switch. (See POWER WINDOW MAIN SWITCH INSPECTION.)
3 | • Measure the voltage at the power window motor. (battery power supply terminal) while operating the passenger’s side power window using the power window main switch. • Is the voltage B+? (Open: terminal A/close: terminal G) | Yes | Go to the next step.
No | Inspect for an open or short circuit in the wiring harness between the power window main switch and the power window motor. Inspect the power window main switch and power window motor connector connections. (damage/pulled-out pins, corrosion) Repair or replace as necessary.
4 | • Operate the passenger’s side power window using the power window main switch. • Does the power window motor operate (rotate)? Caution • If the power window motor temperature is high, the motor may not rotate due to the motor internal bimetal function. Leave it untouched for about 3 min to cool it, then reinspect. | Yes | Go to the next step.
No | Replace the power window motor. (See POWER WINDOW REGULATOR REMOVAL/INSTALLATION.)
5 | • Remove the door glass from carrier plate. • Make sure that the door glass moves smoothly. • Does the door glass move smoothly? | Yes | Replace the power window regulator. (See POWER WINDOW REGULATOR REMOVAL/INSTALLATION.)
No | Inspect for a bent regulator guide or other possible malfunction. If normal, replace the door glass run-channel.