QUICK RELEASE CONNECTOR (EMISSION SYSTEM) CONSTRUCTION/OPERATION [L8, LF]

id0116a3152100

• There are three types of quick release connectors.

Quick release connector locations

amxzzn00000616

Type A

• An SST is not used with this type.
• Mainly consists of a retainer and O-ring. The quick release connector is integrated with the evaporative hose and therefore cannot be disassembled.
• When the quick release connector is connected, the joint port projection is locked at the clamp lock point. By pushing the clamp release tab to expand the clamp, the lock point is released allowing the joint port to be disconnected.

amxzzn00000617

• To connect the quick release connector properly, push it into the joint port until a locking click sound is heard.
• New quick release connectors are fitted with a checker tab that prevents improper fit. This checker tab cannot normally be removed. When the quick release connector is properly connected to the joint port, the lock is released and the checker tab comes off. Due to this, it can be verified that the quick release connector is completely connected.

amxzzn00000618

Type B

• An SST is not used with this type.
• The joint port can be disconnected by squeezing the release tab until the locking tabs release.

e5u116zw5041

• To connect the quick release connector properly, push it into the joint port until a locking click sound is heard.
• New quick release connectors are fitted with a checker tab that prevents improper fit. This checker tab cannot normally be removed. When the quick release connector is properly connected to the connection point, the lock is released and the checker tab comes off. Due to this, it can be verified that the quick release connector is completely connected.

amxzzn00000619

Type C

• Multiple SSTs are used with this type.

amxzzn00000623

amxzzn00000624

• Consists of a retainer and O-ring. The quick release connector is integrated with the evaporative hose and therefore cannot be disassembled.
• To connect the quick release connector properly, push it into the evaporative pipe until a locking click sound is heard.
• New quick release connectors are fitted with a checker tab that prevent improper installation. This checker tab cannot normally be removed. When the quick release connector is properly connected to the evaporative pipe, the lock is released and the checker tab comes off. Due to this, it can be verified that the quick release connector is completely connected.