CONSOLE REMOVAL/INSTALLATION

id091700801200

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the selector lever knob (AT), shift lever knob (MT).

4. Remove in the order indicated in the table.

amxzzw00001412

1 | Parking brake lever boot
2 | Parking brake lever boot plate
3 | Rubber mat
4 | Rear cover
5 | Cup holder guide
6 | Box mat
7 | Power window main switch connector
8 | Indicator compartment connector (AT)
9 | Console

5. Install in the reverse order of removal.