OIL COOLER DISASSEMBLY/ASSEMBLY [SJ6A-EL]

id051311710800

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

e5u513zw5058

1 | Radiator outer tank (in-tank oil cooler) (See Radiator Outer Tank (In-Tank Oil Cooler) Disassembly Note.) (See Radiator Outer Tank (In Tank Oil Cooler) Assembly Note.)
2 | O‐ring
3 | ATF cooler
4 | Radiator

Radiator Outer Tank (In-Tank Oil Cooler) Disassembly Note

1. Inspect the height of the header tabs.

aea5714w079

2. Insert the end of a medium tip screwdriver between the end of the header tab and the outer tank.

  Note
  • Do not open more tabs than necessary for tank removal.

3. Pivot the screwdriver to pry the tab away from the tank and repeat the procedure for each tab.

aea5714w080

  Note
  • If any header tabs are missing from the core, replace the radiator.

4. Remove the radiator outer tank and O‐ring (gasket) from the core header when all of the tabs are opened.

5. Inspect the gasket surface of the radiator core header to ensure it is clean and free of foreign material or damage.

6. Inspect the radiator outer tank for warping. If it is warped, replace the radiator tank.

Radiator Outer Tank (In Tank Oil Cooler) Assembly Note

1. Install a new O‐ring and ensure it is not twisted.

aea5714w081

  Note
  • The old O‐ring must be replaced.

2. Position the radiator tank in the original direction to the core using care not to scratch the tank sealing surface with the header tabs.

  Note
  • Step 3 will set jaw opening to the correct specification.

3. With the jaws of locking‐type pliers (vise grips) closed and locked, turn the adjusting screw to position the jaws against the drill bit with the diameter measured (height) in removal procedure 1. Tighten the lock nut on the adjusting screw against the handle to lock the adjustment in place.

aea5714w082

4. Squeeze the header tabs down in the order as shown in the figure against the lip of the radiator outer tank base with the locking‐type pliers while rotating the pliers toward the tank.

aea5714w083

5. Verify that the height of the header tabs is same as the height before removal.

aea5714w079

6. Inspect for leakage from radiator. (See ENGINE COOLANT LEAKAGE INSPECTION [L8, LF].)