DTC B1342 [ABS]

id0402a7809000

DTC | B1342 | ABS HU/CM system
DETECTION CONDITION | • The ABS HU/CM on-board diagnostic function detects control module malfunction.
POSSIBLE CAUSE | • ABS HU/CM internal malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear the DTC from the memory. (See ON-BOARD DIAGNOSIS [ABS].) • Is same DTC present? | Yes | Replace the ABS HU/CM, then go to the next step. (See ABS HU/CM REMOVAL/INSTALLATION.)
No | Go to the next step.
2 | VERIFY AFTER REPAIR PROCEDURE • Are any other DTCs present? | Yes | Go to the applicable DTC inspection. (See ON-BOARD DIAGNOSIS [ABS].)
No | DTC troubleshooting completed.