SEAT BACK BAR LOWER GARNISH REMOVAL/INSTALLATION

id091700807800

Except Power Retractable Hardtop

1. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

2. Remove the fasteners.

e5u917zw5030

3. Slide the seat back bar lower garnish to the vehicle rear and detach clips A and pin B.

4. Remove the seat back bar lower garnish.

5. Install in the reverse order of removal.

Power Retractable hardtop

1. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (2) Quarter trim (See QUARTER TRIM REMOVAL/INSTALLATION.)

  (3) Scuff plate (See SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

  (5) Aeroboard (See AEROBOARD REMOVAL/INSTALLATION.)

  (6) Seat back bar garnish (See SEAT BACK BAR GARNISH REMOVAL/INSTALLATION.)

  (7) Back trim (See BACK TRIM REMOVAL/INSTALLATION.)

  (8) Roof hook (See ROOF HOOK REMOVAL/INSTALLATION.)

2. Remove the clip A.

amxzzw00001419

3. Remove the roof stopper.

4. Remove the fasteners.

amxzzw00001420

5. Slide the seat back bar lower garnish to the vehicle rear and detach clips B and pin C.

6. Remove the seat back bar lower garnish.

7. Install in the reverse order of removal.