NO.22 NO ENGINE BRAKING [SJ6A-EL]

id050307809600

22 | No engine braking
DESCRIPTION | • Engine speed drops to idle but the vehicle coasts when the accelerator pedal is released during cruising at medium to high speeds. • Engine speed drops to idle but the vehicle coasts when the accelerator pedal is released when in M range (1GR) at low vehicle speed.
POSSIBLE CAUSE | • Clutch slippage, burnt (C4 clutch/B1 brake/B2 brake/B4 brake) ― Line pressure low • VSS malfunction • Improper signal from PCM (engine speed, accelerator pedal position, throttle position, engine coolant temperature, engine torque signals) • Line pressure control solenoid malfunction • Control valve body malfunction Note • Before following the troubleshooting steps, make sure that the Automatic Transmission On-Board Diagnostic and Automatic Transmission Basic Inspection are conducted. (See BASIC INSPECTION [SJ6A-EL].)

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Do the following symptoms occur concurrently? ― Engine flares up or slips during acceleration ― Engine flares up or slips when shifting | Yes | Perform the symptom troubleshooting “NO.14 ENGINE FLARES UP OR SLIPS WHEN UPSHIFTING OR DOWNSHIFTING”, or “NO.15 ENGINE FLARES UP OR SLIPS WHEN ACCELERATING VEHICLE”. (See NO.14 ENGINE FLARES UP OR SLIPS WHEN UPSHIFTING OR DOWNSHIFTING [SJ6A-EL].) (See NO.15 ENGINE FLARES UP OR SLIPS WHEN ACCELERATING VEHICLE [SJ6A-EL].)
No | Go to the next step.
2 | • Access the following PCM PIDs using the M-MDS: (See ON-BOARD DIAGNOSTIC TEST [L8, LF].) ― RPM ― APP ― TP ― ECT • Are the PIDs value normal? (See PCM INSPECTION [L8, LF].) | Yes | Go to the next step.
No | Repair or replace the malfunctioning part according to the inspection results.
3 | • Stop the engine. • Inspect the line pressure control solenoid. (See SOLENOID VALVE INSPECTION [SJ6A-EL].) • Is it normal? | Yes | Inspect the ATF condition. • If a large amount of metal specks are found, overhaul the transmission and repair or replace any malfunctioning parts. (See AUTOMATIC TRANSMISSION REMOVAL/INSTALLATION [SJ6A-EL].) (See Automatic Transmission Workshop Manual [SJ6A-EL].) • If a large amount of metal specks are not found, replace the control valve body. (See CONTROL VALVE BODY REMOVAL [SJ6A-EL].) (See CONTROL VALVE BODY INSTALLATION [SJ6A-EL].)
No | Replace the control valve body. (See CONTROL VALVE BODY REMOVAL [SJ6A-EL].) (See CONTROL VALVE BODY INSTALLATION [SJ6A-EL].)
4 | • Verify test results. ― If normal, return to the diagnostic index to service any additional symptoms. ― If malfunction remains, inspect the related Service Information and perform repair or diagnosis. • If the vehicle is repaired, troubleshooting completed. • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM. (See TCM REMOVAL/INSTALLATION [SJ6A-EL].)