ENGINE OIL LEVEL INSPECTION [L8, LF]

id0111c6800500

1. Position the vehicle on level ground.

2. Warm up the engine.

3. Stop the engine and allow at least 5 min before continuing.

4. Remove the dipstick, wipe it cleanly, and reinstall it fully.

5. Remove the dipstick and verify that the oil level is between the F and L marks on the dipstick.

  • If the oil level is below the L mark, add engine oil.

  amxzzw00001952