TRANSMISSION OIL INSPECTION [P66M-D]

id051111247800

1. Position the vehicle on level ground.

2. Remove the Insulator. (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)

3. Remove oil filler plug.

amxzzw00000516

4. Verify that the oil is near the brim of the plug port.

  • If the oil is not near the brim of the plug port, add the specified amount and type of oil.

  Transmission case specified oil grade

  API service GL-4 or GL-5

  Transmission case specified oil viscosity

  SAE 75W-90

5. Install oil filler plug and a new washer.

  Tightening torque

  40—59 N·m {4.1—6.0 kgf·m, 30—43 ft·lbf}

6. Install the Insulator. (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)