CONTROL VALVE BODY REMOVAL [SJ6A-EL]

id051311710600

On-Vehicle Removal

  Warning
  • A hot transmission and ATF can cause severe burns. Turn off the engine and wait until they are cool before replacing ATF.
  • Using compressed air can cause dirt and other particles to fly out, causing injury to the eyes. Wear protective eye wear whenever using compressed air.

  Caution
  • Clean the transmission exterior thoroughly with a stream cleaner or cleaning solvents before removal.
  • If any old sealant gets into the transmission during installation of the oil pan, trouble may occur in the transmission case and oil pan. Clean with cleaning fluids.

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Drain the ATF. (See AUTOMATIC TRANSMISSION FLUID (ATF) REPLACEMENT [SJ6A-EL].)

  Caution
  • Do not damage the fitting surface of the transmission case and the oil pan.
  • Do not to deform the oil pan.

4. Remove the oil pan and the oil pan gasket.

5. Remove the magnets from the oil pan.

amxzzw00000149

  Note
  • Examine the chips and particles in the oil pan to determine what type of wear has occurred in the transmission. Steel (magnetic)= bearing, gear and plate wear. Brass (non-magnetic)= busing wear.

6. Remove the oil strainer from the control valve body component.

e5u513zw5048

7. Remove the O-ring from the oil strainer.

8. Disconnect the connectors from the solenoids.

amxzzw00000773

9. Disconnect the coupler component from the clamps.

10. Remove the lock plate from the control valve body component.

e5u513zw5067

11. Pull the TFT sensor from the control valve body component.

  Note
  • Be sure that the coupler component does not interface with the control valve body component when installing.

12. Fix the coupler component with tape to the transmission case as shown in the figure.

e5u513zw5050

13. Remove the detent spring cover and detent spring from the control valve body component.

e5u513zw5047

14. Remove the bolts from the transmission case as shown in the figure.

amxzzw00000150

  Caution
  • Do not to drop the control valve body component.

15. Disconnect the manual valve link and remove the control valve body component.

e5u513zw5072

16. Remove the check valve sub-component and the compression spring from the transmission case.

amxzzw00000151

17. Remove the transmission case gaskets and the brake drum gaskets from the transmission case.

amxzzw00000152

  Caution
  • Take care as the C-2 and B-3 accumulator piston may eject.

18. Apply compressed air into the oil passage as shown in the figure and remove the accumulator pistons (C-2, B-3) and the compression springs from the transmission case.

amxzzw00000153

  Caution
  • Do not to damage the accumulator pistons.

19. Remove the snap rings from the accumulator pistons (C-2, B-3) using a flathead screwdriver.

20. Remove the compression springs from the accumulator pistons (C-2, B-3).

21. Remove the O-rings from the accumulator pistons (C-2, B-3) using a flathead screwdriver.

  Caution
  • Take care as the C-3 accumulator piston may eject.

22. Apply compressed air into the oil passage as shown in the figure and remove the accumulator piston (C-3) and compression springs from the transmission case.

amxzzw00000154

23. Remove the O-rings from the accumulator piston (C-3) using a flathead screwdriver.

24. Remove the accumulator valve and compression springs from the transmission case.

amxzzw00000155