DTC TABLE [INSTRUMENT CLUSTER]

id0902e8960500

DTC | Description | Page
--- | --- | ---
B1213 | Only one key ID number is registered. | (See SECURITY LIGHT 21, DTC B1213/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B1342 | Instrument cluster malfunction | (See DTC B1342 [INSTRUMENT CLUSTER].)
B1600 | The key ID number data cannot be read. | (See SECURITY LIGHT 13, DTC B1600/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B1601 | The instrument cluster has detected unregistered key ID number. | (See SECURITY LIGHT 15, DTC B1601/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B1602 | The instrument cluster cannot read key ID number data normally. | (See SECURITY LIGHT 14, DTC B1602/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B1681 | No detected communication with the coil antenna | (See SECURITY LIGHT 11, DTC B1681/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2103 | • Coil antenna malfunction • The PCM determined a malfunction in the coil antenna even though it is normal. | (See SECURITY LIGHT 12, DTC B2103/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2139 | ID number data in the PCM and the instrument cluster do not match. | (See SECURITY LIGHT 23, DTC B2139/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2141 | Communication error between the instrument cluster and the PCM (data transfer error) | (See SECURITY LIGHT 22, DTC B2141/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2431 | Key ID number registration error | (See SECURITY LIGHT 13, DTC B2431/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)
B2477 | Instrument cluster configuration not performed | (See DTC B2477 [INSTRUMENT CLUSTER].)
B2840 | Ambient temperature sensor circuit malfunction | (See DTC B2840 [INSTRUMENT CLUSTER].)
U0028 | Invalid data received from climate control unit | (See DTC U0028 [INSTRUMENT CLUSTER].)
U0073 | HS-CAN Bus off | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0100 | Communication error to PCM
U0101 | Communication error to TCM
U0121 | Communication error to ABS
U0127 | Communication failure between instrument cluster and keyless receiver | (See DTC U0127.)
U0207 | Communication error to power retractable hardtop control module | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0214 | Communication error to keyless control module
U0250 | Communication error to active bonnet control module
U2023 | Abnormal message from PCM | (See DTC U2023 [INSTRUMENT CLUSTER].)
U2064 | Warning light illumination request signal from other modules | (See DTC U2064 [INSTRUMENT CLUSTER].)
U2197 | Vehicle speed signal communication error | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U2510 | Communication error between the instrument cluster and the PCM (no response) | (See SECURITY LIGHT 16, DTC U2510/P1260, U1147/P1260 [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)].)