AUTO LEVELING CONTROL MODULE REMOVAL/INSTALLATION

id091800473200

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the glove compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

4. Disconnect the connector.

amxzzw00001090

5. Remove the bolt and then remove the auto leveling control module.

6. Install in the reverse order of removal.