TRANSMISSION OIL REPLACEMENT [P66M-D]

id051111247900

1. Position the vehicle on level ground.

2. Remove the Insulator. (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)

3. Remove oil filler plug and drain plug, and then drain the oil.

amxzzw00000517

4. Clean drain plug.

5. Install drain plug and a new washer.

  Tightening torque

  40—59 N·m {4.1—6.0 kgf·m, 30—43 ft·lbf}

6. Add the specified amount and type of oil through the plug port for oil filler plug to near the brim of the port.

amxzzw00000518

  Transmission case specified oil grade

  API service GL-4 or GL-5

  Transmission case specified oil viscosity

  SAE 75W-90

  Transmission case capacity (approx. quantity)

  2.1 L {2.2 US qt, 1.8 lmp qt}

7. Install oil filler plug and a new washer.

amxzzw00000519

  Tightening torque

  40—59 N·m {4.1—6.0 kgf·m, 30—43 ft·lbf}

8. Install the Insulator. (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)