BRAKES TECHNICAL DATA

id045000800100

Item | Specification
--- | ---
Brake fluid type | European (L.H.D. U.K.) specs: SAE J1703, FMVSS 116 DOT-3 or DOT-4 Australian, General (L.H.D.) specs: SAE J1703, FMVSS 116 DOT-3
Brake pedal height (reference value) | 167 mm {6.57 in}
Brake pedal play | 2—5 mm {0.08—0.19 in}
Brake pedal-to-floor clearance (Brake pedal when depressed at 147 N {15.0 Kgf, 33.0 lbf} | 106.9 mm {4.209 in} or more
Front disc plate runout limit | 0.05 mm {0.002 in}
Minimum front disc plate thickness | 20 mm {0.79 in}
Minimum front disc plate thickness after machining using a brake lathe on-vehicle | 20.8 mm {0.82 in}
Minimum front disc pad thickness | 2.0 mm {0.079 in} min.
Rear disc plate runout limit | 0.05 mm {0.002 in}
Minimum rear disc plate thickness | 8 mm {0.31 in}
Minimum rear disc plate thickness after machining using a brake lathe on-vehicle | 8.8 mm {0.35 in}
Minimum rear disc pad thickness | 2.0 mm {0.079 in} min.
Parking brake lever stroke when pulled at 98 N {10 kgf, 22 lbf} | 1—3 notches

Power brake unit fluid pressure

Vacuum amount at o kPa {0 mmHg, 0 inHg}
Pedal force (N {kgf, lbf}) | Fluid pressure (kPa {kgf/cm2, psi})
--- | ---
200 {20.4, 44.9} | 620 {6.33, 90.0} or more

Power brake unit fluid pressure

Vacuum amount at o 66.7 kPa {500 mmHg, 19.7 inHg}
Pedal force (N {kgf, lbf}) | Fluid pressure (kPa {kgf/cm2, psi})
--- | ---
200 {20.4, 44.9} | 6,340 {64.65, 919.6} or more