LOAD LIMITER RETRACTOR CONSTRUCTION/OPERATION

id081100100300

1. Initial state

amxzzn00000653

2. ELR operation

When the force of impact is transfered to the belt, the retractor changes to the ELR condition, locking the belt and securing the passenger’s body.

amxzzn00000391

3. Load limiter operation

After locking, if the force of impact transferred to the belt is strong enough to cause injury to the chest of the occupant, an adequate amount of belt is released to absorb the load applied to the chest.

amxzzn00000654