PRE-DELIVERY INSPECTION

id000000801100

Pre-Delivery Inspection Table

Exterior

INSPECT and ADJUST, if necessary, the following part to specification:
qGlass, exterior bright metal and paint for damage
qConvertible top for damage
qPower retractable hardtop for damage
qWheel lug nuts
qAll weatherstrips for damage or detachment
qOperation of bonnet release and lock
qOperation of trunk lid and fuel-filler lid
qDoor operation and alignment
qHeadlight aiming
TRUNK ROOM
qInspect operation of trunk lid internal release
INSTALL the following part:
qWheel caps (if equipped)
qMast antenna (if equipped)

Under bonnet—engine off

INSPECT and ADJUST, if necessary, the following part to specification:
qFuel, engine coolant, and hydraulic lines, fittings, connections, and components for leaks
qEngine oil level
qPower steering fluid level
qBrake and clutch master cylinder fluid level
qWasher tank fluid level
qAutomatic transmission fluid level
qRadiator coolant level and specific gravity
qTightness of battery terminals

Interior

INSPECT the operations of the following part:
qSeat controls (slide and recline)
qSeat belts and warning system
qAir bag system using warning light
qCruise control system (if equipped)
qIgnition switch and steering lock
qStarter interlock (if equipped)
qPower door lock
qDoor locks
qAll lights including warning, and indicator lights
qHorn, wipers, and washers
qWiper blades performance
qAudio system
qPower windows (if equipped)
qHeater, defroster, and air conditioner at various mode selections (if equipped)
INSPECT the following part:
qPresence of spare fuse
qUpholstery and interior finish
INSPECT and ADJUST, if necessary, the following part:
qPedal height and free play of brake and clutch pedal
qParking brake

Under bonnet—engine running at operating temperature

INSPECT the following part:
qAutomatic transmission fluid level

On hoist

INSPECT the following part:
qUnderside fuel, coolant and hydraulic lines, fittings, connections, and components for leaks
qTires for cuts or bruises
qSteering linkage, suspension, exhaust system, and all underside hardware for looseness or damage
qManual transmission oil level
qDifferential oil level

Road test

INSPECT the following part:
qBrake operation
qClutch operation
qSteering control
qEmergency locking retractors and automatic locking retractors
qCruise control system (if equipped)
qOperation of meters and gauges, squeaks, rattles, and unusual noises

After road test

INSPECT for necessary owner information materials, tools, and spare tire in vehicle
The following part must be completed just before delivery to your customer.
qLoad test battery and charge if necessary (Load test result: Volts)
qAdjust tire pressure to specification
qClean outside of vehicle
qInstall fuses for accessories
qRemove seat and cabin carpet protective covers
qVacuum inside of vehicle
qInspect installation of option parts with invoice