ELECTRONIC CONTROL ITEMS AND CONTENTS [SJ6A-EL]

id051311324800

Item | Content
--- | ---
Shift control | • Detects engine load and vehicle speed, and switches to optimum gear in accordance with preset shift program. • In D range, automatically switches between NORMAL, AAS, DOWN-SLOPE, UP-SLOPE modes according to specific conditions.
Manual mode shift control | • Shifts to selected gear position by manual shifting of the selector lever forward and back. • The up/down operation of the steering shift switch is the same as the manual operation of the selector lever.
Direct mode control | • Shifts temporarily by using the steering shift switch even when the selector lever is in the D range
TCC control | • According to preset TCC point, performs TCC operation.
5-6 shift inhibit control | • Inhibits shift change from the 5th to 6th gears when the engine is cold.
Torque reduction control | • Optimally controls engine output torque when shifting.
Line pressure control | • Controls line pressure according to driving conditions.
Shift learning control | • Performs optimal correction for clutch engagement pressure to reduce changes in engine performance and/or elapsed transmission.
On-board diagnostic system | • Detects and/or memorizes failure of input/output part and transmission condition.