AIRFLOW TEMPERATURE CONTROL OPERATION [FULL-AUTO AIR CONDITIONER]

id0740a1102300

Airflow Temperature Automatic Control

• The climate control unit calculates the air mix actuator angle (airflow temperature) by correcting the target temperature, which is calculated from the setting temperature and the input from each sensor, with the input from the engine coolant temperature sensor and evaporator temperature sensor, and each mode to operate the actuator.

amxzzn00000349