SOLAR RADIATION SENSOR REMOVAL/INSTALLATION [FULL-AUTO AIR CONDITIONER]

id0740a1802800

1. Remove the battery cable.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Pry the solar radiation sensor from the dashboard using a flathead screwdriver wrapped with protective tape.

4. Remove in the order indicated in the table.

amxzzw00000978

1 | Solar radiation sensor connector
2 | Solar radiation sensor

5. Install in the reverse order of removal.