PCM REMOVAL/INSTALLATION [L8, LF]

id0140i7802400

1. When replacing the PCM, perform the following:

  • PCM configuration (See PCM CONFIGURATION [L8, LF].)

2. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove the air cleaner case. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)

5. Move the water hose from the PCM cover slightly out of the way.

6. Remove in the order indicated in the table.

Except for U.K. specs.

amxzzw00000019

1 | PCM cover
2 | PCM connector (See PCM Connector Connection Note.)
3 | PCM
4 | Air cleaner insulator
5 | PCM duct

U.K. specs.

amxzzw00000020

1 | Set bolt (See Set Bolt Removal Note.) (See Set Bolt Installation Note.)
2 | PCM cover
3 | PCM connector (See PCM Connector Connection Note.)
4 | PCM
5 | PCM bracket
6 | Air cleaner insulator
7 | PCM duct

7. Install in the reverse order of removal.

8. When replacing the PCM on the vehicles, perform the following:

  • PCM parameter reset (See IMMOBILIZER SYSTEM-RELATED PARTS PROGRAMMING.)

Set Bolt Removal Note

1. Using a chisel and a hammer, cut a groove on the head of the set bolt so that a screwdriver can be inserted.

2. Loose the set bolt using an impact screwdriver or pliers.

amxzzw00000021

PCM Connector Connection Note

  Caution
  • If the PCM connector is inserted at an angle and the lever is moved, the connector could be damaged. Verify that the PCM connector is inserted straight.

  acxaaw00000768

1. Verify that the PCM connector lever is tilted towards the wiring harness side as shown in the figure.

acxaaw00000766

2. Insert the PCM connector straight until it contacts the PCM and verify that the lever reverts upward naturally.

3. Push the lever until a click is heard.

acxaaw00000767

Set Bolt Installation Note

1. Install a new set bolt and tighten it until the neck of the bolt is cut.

amxzzw00000022