KEYLESS CONTROL MODULE REMOVAL/INSTALLATION

id091400438400

  Note
  • If the keyless control module is replaced, always perform the following procedure.
    ― Immobilizer system resetting (with immobilizer system) (See IMMOBILIZER SYSTEM-RELATED PARTS PROGRAMMING.)

L.H.D.

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the side panel. (See SIDE PANEL REMOVAL/INSTALLATION.)

3. Remove the bolt and nut.

amxzzw00000571

4. While inclining the keyless control module along the body panel in the direction indicated by the arrow, disengage the bracket tab from the hole in the body panel.

5. Disconnect the keyless control module connector.

6. Remove the keyless control module.

7. Remove the screw, then remove the bracket.

e6u914zw1006

  Note
  • The screw which fixes the keyless control module and bracket is for a body ground connection. Be sure to secure the screw when installing.

8. Install in the reverse order of removal.

R.H.D.

  Note
  • Disconnect the fuse block and the vehicle wiring harnesses, and then remove them to secure a work space.

  amxzzw00000572

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the keyless control module installation bolt and nut.

amxzzw00000573

3. Remove the side panel. (See SIDE PANEL REMOVAL/INSTALLATION.)

4. Insert a flathead screwdriver between the bracket and the body from the installation hole of the side cover and move it in the direction shown by the arrow to remove the keyless control module.

amxzzw00000574

  Note
  • If the bracket is deformed, repair it.
  • Bend the tab straight as shown in the figure for easier installation access.

  amxzzw00000575

5. Remove the keyless control module.

6. Remove the screw, then remove the bracket.

e6u914zw1006

  Note
  • The screw which fixes the keyless control module and bracket is for a body ground connection. Be sure to secure the screw when installing.

7. Install in the reverse order of removal.