REARVIEW MIRROR REMOVAL/INSTALLATION

id091200803100

Type A

1. Remove the cover.

e5u912zw5028

2. Depress the clip, and then remove the rearview mirror by pulling upward.

e5u912zw5029

3. Install in the reverse order of removal.

Type B

1. Insert a flathead screwdriver between the mirror and the base.

amxzzw00000720

2. Push the base pin down to remove the rearview mirror.

3. Install the rearview mirror onto the base.

amxzzw00000721