KEYLESS RECEIVER INSPECTION

id091400437800

1. Measure the voltage or inspect for continuity according to the Terminal Voltage Table (Reference).

  • If the voltage is not as specified in the Terminal Voltage Table (Reference), inspect the parts under “Inspection item(s)” and related wiring harnesses.

Terminal Voltage Table (Reference)

e6u914zw1007

Terminal | Signal name | Connected to | Measured condition | Voltage (V)/Continuity | Inspection item(s)
--- | --- | --- | --- | --- | ---
A | Power supply | Keyless control module | Under any condition | B+ | • Keyless control module • Related wiring harnesses
C | Data | Keyless control module | Under any condition: Inspect the wiring harness between the keyless receiver and keyless control module terminal 3U for continuity. | Continuity detected | • Keyless control module • Related wiring harnesses
E | GND | Body ground | Under any condition: Inspect for continuity to ground. | Continuity detected | GND