SELECTOR LEVER STRUCTURE

id051400328200

M Range Switch

Outline

  • The M range switch detects the selector lever in M range position and sends a manual mode request signal to the TCM.

  L.H.D.

  amxzzn00000070

  R.H.D.

  amxzzn00000071

Operation

  • The M range switch is an ON/OFF type switch that turns on when the selector lever is shifted to the M range. It also remains on during up-shift and down-shift operations.

Up Switch

Outline

  • The up switch detects an up-shift operation in the M range and sends an up-shift request signal to the TCM.

  L.H.D.

  amxzzn00000072

  R.H.D.

  amxzzn00000073

Operation

  • The up switch is an ON/OFF type switch that turns on when the selector lever is in the M range (+) side position.

Down Switch

Outline

  • The down switch detects a down-shift operation in the M range and sends a down-shift request signal to the TCM.

  L.H.D.

  amxzzn00000074

  R.H.D.

  amxzzn00000075

Operation

  • The down switch is an ON/OFF type switch that turns on when the selector lever is in the M range (–) side position.