DSC OFF SWITCH REMOVAL/INSTALLATION

id041500801900

1. For L.H.D., remove the side panel. (See SIDE PANEL REMOVAL/INSTALLATION.)

2. For R.H.D., remove the lower panel. (See LOWER PANEL REMOVAL/INSTALLATION.)

3. For R.H.D., remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

amxzzw00002746

1 | DSC OFF switch connector (See DSC OFF Switch Connector Removal Note.)
2 | DSC OFF switch (See DSC OFF Switch Removal Note.)

5. Install in the reverse order of removal.

DSC OFF Switch Connector Removal Note

1. Access the DSC OFF switch connector from behind of the dashboard, and squeeze the tabs of the switch connector.

2. Disconnect the DSC OFF switch connector from the DSC OFF switch.

DSC OFF Switch Removal Note

1. Access the DSC OFF switch from behind of the dashboard, and squeeze the tabs of the switch.

2. Pull the DSC OFF switch towards the driver’s side to remove it.