ENGINE MOUNTING/DISMOUNTING

id011000507000

1. Install the SSTs (arms) to the cylinder block holes as shown, and hand-tighten the bolts (part No.: 9YA20-1003) or M10 × 1.5T length 90 mm {3.55 in}.

belbze00000030

2. Assemble the SSTs (bolts, nuts and plate) to the specified positions.

belbze00000031

3. Adjust the SSTs (bolts) so that less than 20 mm {0.79 in} of thread is exposed.

4. Make the SSTs (arms and plate) parallel by adjusting the SSTs (bolts and nuts).

5. Tighten the SSTs (bolts and nuts) to affix the SSTs firmly.

belbze00000032

  Warning
  • Self-locking brake system of the engine stand may not be effective when the engine is held in an unbalanced position. This could lead to sudden, rapid movement of the engine and mounting stand handle and cause serious injury. Never keep the engine in an unbalanced position, and always hold the rotating handle firmly when turning the engine.

6. Mount the engine on the SST (engine stand).

7. Drain the engine oil into a container.

8. Install the oil pan drain plug.

  • With washer
    1. Install the oil pan drain plug with a new washer.

  Tightening torque

  30—41 N·m {3.1—4.1 kgf·m, 23—30 ft·lbf}

  • Without washer
    1. Inspect the seal rubber of the oil pan drain plug and make sure there are no cracks or damage.
      ― If necessary, replace the oil pan drain plug.
    2. Clean the flange surface (seal rubber) on the oil pan drain plug, then install the oil pan drain plug.

  Tightening torque

  22—30 N·m {2.2—3.1 kgf·m, 16—22 ft·lbf}

DISMOUNTING

• Dismount in the reverse order of mounting.