FRONT SIDE FRAME (PARTIAL CUTTING) INSTALLATION [PANEL REPLACEMENT]

id098008742200

  Caution
  • The cut-and-joint area indicates the maximum size range of the installation position.

1. Make a reinforcement panel using the material from the front side frame.

2. To cut and join the new and existing parts, cut the new part at the specified location shown in the figure, and chamfer the joint surfaces of the new and existing parts.

3. When installing the new parts, trial-fit new and existing parts, and then measure and adjust the body to conform with standard dimensions.

4. After temporarily installing new parts, make sure the related parts fit properly.

5. Trial-fit the new and existing parts, weld the existing parts and the reinforcement, and then butt weld the new and existing parts.

  Caution
  • Press fit the reinforcement panel and the body side material, and then continuous weld them.

amxzzb00000021