FRONT AUTO LEVELING SENSOR INSPECTION

id091800474000

1. Connect three 1.5 V dry cell batteries in a series.

amxzzw00001077

2. Connect the positive pole of the battery to front auto leveling sensor terminal A, and the negative pole to terminal D, then apply voltage of 4.5 V between terminals A and D.

3. Connect the tester as shown in the figure.

4. Measure the voltage while the link is moved up and down slowly.

  • If not as indicated in the table, replace the front auto leveling sensor.

Link angle (vehicle height) | Voltage (V)
--- | ---
+28° (High) | 3.4
0° | 2.3
-26° (Low) | 1.2