MANUAL ANTENNA INSPECTION

id092000807700

  Note
  • A amplifier is built into the manual antenna.

Antenna Amplifier

1. Turn on the audio unit and radio, and measure the voltage at manual antenna connector terminal C.

e5u920zw5303

  • If the voltage is B+, inspect the antenna feeder.
  • If the voltage is not B+, inspect the audio unit or the antenna feeder.

Manual Antenna

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the manual antenna connector.

4. Inspect for continuity between the manual antenna terminals using an ohmmeter.

amxzzw00001682

  • If not as specified, replace the manual antenna.

e5u920zw5122