POWER OUTER MIRROR SWITCH REMOVAL/INSTALLATION

id091200420400

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the handle pull. (See DOOR TRIM DISASSEMBLY/ASSEMBLY.)

4. Remove the armrest. (See DOOR TRIM DISASSEMBLY/ASSEMBLY.)

5. Remove the door trim. (See DOOR TRIM REMOVAL/INSTALLATION.)

6. Remove the switch panel from the door trim by depressing the tab.

e5u912zw5025

7. Remove the screws and the power outer mirror switch.

8. Install in the reverse order of removal.