DTC TABLE [SJ6A-EL]

id050208800500

X: Available
–: N/A

DTC No. | Condition | MIL | AT warning light | DC | Memory function | Page
--- | --- | --- | --- | --- | --- | ---
P0601 | Flash ROM malfunction | X | X | 1 | X | (See DTC P0601 [SJ6A-EL])
P0603 | EEPROM malfunction | X | X | 1 | X | (See DTC P0603 [SJ6A-EL])
P0604 | RAM malfunction | X | X | 1 | X | (See DTC P0604 [SJ6A-EL])
P0707 | Transmission range (TR) switch circuit low input (short to ground) | X | X | 1 | X | (See DTC P0707 [SJ6A-EL])
P0708 | Transmission range (TR) switch circuit high input (open circuit) | X | X | 2 | X | (See DTC P0708 [SJ6A-EL])
P0711 | Transmission fluid temperature (TFT) sensor malfunction (stuck) | X | X | 2 | X | (See DTC P0711 [SJ6A-EL])
P0712 | Transmission fluid temperature (TFT) sensor circuit malfunction (short to ground) | X | X | 1 | X | (See DTC P0712 [SJ6A-EL])
P0713 | Transmission fluid temperature (TFT) sensor circuit malfunction (short to power/open circuit) | X | X | 1 | X | (See DTC P0713 [SJ6A-EL])
P0717 | Turbine sensor circuit malfunction (open circuit/short circuit) | X | X | 1 | X | (See DTC P0717 [SJ6A-EL])
P0722 | Vehicle speed sensor (VSS) circuit malfunction (open circuit/short circuit) | X | X | 1 | X | (See DTC P0722 [SJ6A-EL])
P0751 | Shift solenoid A malfunction (stuck off) | X | X | 2 | X | (See DTC P0751 [SJ6A-EL])
P0752 | Shift solenoid A malfunction (stuck on) | X | X | 2 | X | (See DTC P0752 [SJ6A-EL])
P0756 | Shift solenoid B malfunction (stuck off) | X | X | 2 | X | (See DTC P0756 [SJ6A-EL])
P0757 | Shift solenoid B malfunction (stuck on) | X | X | 2 | X | (See DTC P0757 [SJ6A-EL])
P0761 | Shift solenoid C malfunction (stuck off) | X | X | 2 | X | (See DTC P0761 [SJ6A-EL])
P0762 | Shift solenoid C malfunction (stuck on) | X | X | 2 | X | (See DTC P0762 [SJ6A-EL])
P0766 | Shift solenoid D malfunction (stuck off) | X | X | 2 | X | (See DTC P0766 [SJ6A-EL])
Shift solenoid G malfunction (stuck on) | X | X | 2 | X | (See DTC P0766 [SJ6A-EL])
P0781 | 1-2 shift valve malfunction | X | X | 2 | X | (See DTC P0781 [SJ6A-EL])
P0813 | Reverse sequence valve malfunction | X | X | 2 | X | (See DTC P0813 [SJ6A-EL])
P0819 | Manual switch/up switch/down switch circuit malfunction (open circuit/short circuit) | – | X | 1 | X | (See DTC P0819 [SJ6A-EL])
P0826 | Steering shift switch circuit malfunction (open circuit/short to ground) | X | X | 1 | X | (See DTC P0826 [SJ6A-EL])
P0882 | TCM B+ low (less than 9 V) | X | X | 1 | X | (See DTC P0882 [SJ6A-EL])
P0961 | Line pressure control solenoid range/performance (stuck) | X | X | 1 | X | (See DTC P0961 [SJ6A-EL])
P0962 | Line pressure control solenoid circuit malfunction (short to ground/open circuit) | X | X | 1 | X | (See DTC P0962 [SJ6A-EL])
P0963 | Line pressure control solenoid circuit malfunction (short to power) | X | X | 1 | X | (See DTC P0963 [SJ6A-EL])
P0969 | Shift solenoid F range/performance (stuck) | X | X | 1 | X | (See DTC P0969 [SJ6A-EL])
P0970 | Shift solenoid F circuit malfunction (short to ground/open circuit) | X | X | 1 | X | (See DTC P0970 [SJ6A-EL])
P0971 | Shift solenoid F circuit malfunction (short to power) | X | X | 1 | X | (See DTC P0971 [SJ6A-EL])
P0973 | Shift solenoid A circuit malfunction (short to ground) | X | X | 1 | X | (See DTC P0973 [SJ6A-EL])
P0974 | Shift solenoid A circuit malfunction (short to power/open circuit) | X | X | 1 | X | (See DTC P0974 [SJ6A-EL])
P0976 | Shift solenoid B circuit malfunction (short to ground) | X | X | 1 | X | (See DTC P0976 [SJ6A-EL])
P0977 | Shift solenoid B circuit malfunction (short to power/open circuit) | X | X | 1 | X | (See DTC P0977 [SJ6A-EL])
P0979 | Shift solenoid C circuit malfunction (short to ground) | X | X | 1 | X | (See DTC P0979 [SJ6A-EL])
P0980 | Shift solenoid C circuit malfunction (short to power/open circuit) | X | X | 1 | X | (See DTC P0980 [SJ6A-EL])
P0982 | Shift solenoid D circuit malfunction (short to ground) | X | X | 1 | X | (See DTC P0982 [SJ6A-EL])
P0983 | Shift solenoid D circuit malfunction (short to power/open circuit) | X | X | 1 | X | (See DTC P0983 [SJ6A-EL])
P0985 | Shift solenoid E circuit malfunction (short to ground) | X | X | 1 | X | (See DTC P0985 [SJ6A-EL])
P0986 | Shift solenoid E circuit malfunction (short to power/open circuit) | X | X | 1 | X | (See DTC P0986 [SJ6A-EL])
P2719 | Shift solenoid G range/performance (stuck) | X | X | 1 | X | (See DTC P2719 [SJ6A-EL])
P2720 | Shift solenoid G circuit malfunction (short to ground/open circuit) | X | X | 1 | X | (See DTC P2720 [SJ6A-EL])
P2721 | Shift solenoid G circuit malfunction (short to power) | X | X | 1 | X | (See DTC P2721 [SJ6A-EL])
P2757 | Torque converter clutch (TCC) stuck off | X | X | 2 | X | (See DTC P2757 [SJ6A-EL])
P2758 | Torque converter clutch (TCC) stuck on | X | X | 2 | X | (See DTC P2758 [SJ6A-EL])
P2762 | TCC control solenoid range/performance (stuck) | X | X | 1 | X | (See DTC P2762 [SJ6A-EL])
P2763 | TCC control solenoid circuit malfunction (short to power) | X | X | 1 | X | (See DTC P2763 [SJ6A-EL])
P2764 | TCC control solenoid circuit malfunction (short to ground/open circuit) | X | X | 1 | X | (See DTC P2764 [SJ6A-EL])
U0073 | CAN BUS OFF | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)]) (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)])
U0100 | TCM cannot receive any signals from PCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)]) (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)])

MIL : Malfunction Indicator Lamp
DC : Drive Cycle
– : N/A