FOREWORD [SJ6A-EL]

id050208800200

• When the customer reports vehicle malfunction, check the malfunction indicator lamp (MIL) indication, AT warning indication, and diagnostic trouble code (DTC), then diagnose the malfunction according to following flowchart.

  ― If a DTC exists, diagnose the applicable DTC inspection. (See DTC TABLE [SJ6A-EL].)
  ― If a DTC does not exist and the MIL and AT warning lights do not illuminate, diagnose the applicable symptom troubleshooting. (See SYMPTOM TROUBLESHOOTING ITEM TABLE [SJ6A-EL].)

amxzzw00000172

*: Malfunction Indicator Lamp (MIL), AT warning light