TRANSVERSE MEMBER REMOVAL/INSTALLATION

id021300801100

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

amxuuw00001908

1 | Under cover (See Under Cover Installation Note.)
2 | Transverse member (See Transverse Member Removal Note.)

Transverse Member Removal Note

1. Support the crossmember using a jack.

2. Remove the transverse member.

Under Cover Installation Note

1. Align projection A with the transverse member opening to temporarily support the under cover.

e5u213zw5017

2. Tighten the bolts in the order of A, B and C.

e5u213zw5018